**GEO5 Field Tests Import: Step-by-Step Guide**

1. **Open the GEO5 Module**  
   In your GEO5 project (typically the Stratigraphy module), go to the **Field Tests** frame.
2. **Import Field Test Data**  
   Click **Import** and select **Spreadsheets**.  
   Choose the **Geo5\_Import.xlsx** file that you have downloaded.  
   In the import menu, **set the template** for each field test to:  
   **EN - Standard: Borehole**

A screenshot of a computer

AI-generated content may be incorrect.

1. **Adopt Borehole Data**  
   Once import is complete, head to the **Soils** frame.  
   Click **Adopt from field tests** to transfer field test soil layers into the model.
2. **Specify Soil Properties**  
   Enter soil parameters and assign colour coding as needed.
3. **Create Sections and Use Other Utilities**  
   To create sections or use additional tools, go to the **Geological Model** frame and select **Generate**.